1.0-1.2t EXCAVATOR

|  |
| --- |
| Main Technical Specification |
| Dimension |
| Wheel Tread | mm | 910 |
| Length of track | mm | 1230 |
| Ground clearance of upper platform | mm | 380 |
| Turning radius of tail | mm | 735 |
| Width | mm | 1130 |
| Width of track | mm | 180 |
| Height of track | mm | 320 |
| Length | mm | 2650 |
| Height | mm | 2200 |
| Driving speed | Km/h | 0-2km/h |
| Operating range |
| Maximum digging radius | mm | 2850 |
| Maximum digging depth | mm | 1650 |
| Maximum digging height | mm | 2610 |
| Maximum vertical digging depth | mm | 1375 |
| Maximum swing radius | mm | 1330 |
| Height of bulldozing plate | mm | 345 |
| Depth of bulldozing plate | mm | 255 |
| Engine | KOOP (KD192) Euro V |
| Engine power | kw | 8.6 |
| Operation weight | kgs | 1200 |
| Bucket capacity | m³ | 0.02 |
| **1.2ton with much stronger structure canopy** |